The ISIS

OPEN G ENIE

User Manual

F A Akeroyd R L Ashworth S D Johnston J M Martin C M Moreton-Smith D S Sivia

version 1.1

Forward

This manual should enable you to become familiar withOpen GENIE quickly and easily. It therefore complements theOpen GENIE Reference Manual which should be used to understand the full meaning of Open GENIE commands. The reference manual is accessible on the ISIS web server at:

• http://www.isis.rl.ac.uk/GENIEReferenceManual/

and the user manual is planned to be accessible by January �98 at

• http://www.isis.rl.ac.uk/GENIEUserManual/

The Open GENIE User Manual is separated into two parts:

• Part A . The User Manual

An introduction to the use of Open GENIE

• Part B . The Installation Guide

General information on how to install and run Open GENIE.

Assuming that you are new toOpen GENIE and have just downloaded a copy you will need to consult the Installation Guide to get Open GENIE installed on your machine.

After this we recommend you experiment with some of the example files to get an idea of the capabilities of Open GENIE.

For further information, comments, additions of routines that you feel should be included, please contact us at genie@isise.rl.ac.uk.

To be kept up to date with new releases send a message togenie-announce-request@isise.rl.ac.uk with no subject, and the body of the message containing the two lines, - this will add you to the mailing list

SUBSCRIBE

QUIT

Table of contents

FORWARD ...................................................................................................................I

TABLE OF CONTENTS ...........................................................................................II

PART A - USER MANUAL ........................................................................................1 WHAT IS OPEN GENIE ?.............................................................................................1 GETTING STARTED...................................................................................................... 1 STARTING UP OPEN GENIE..........................................................................................2 Remote operation of Open GENIE at ISIS.............................................................2

a) Via Telnet .............................................................................................................................. 2 b) Via a terminal emulator ......................................................................................................... 2

A FEW USEFUL FACTS ABOUTOPEN GENIE................................................................3 Commands.............................................................................................................3 Data types ..............................................................................................................4 Operations .............................................................................................................6 File names..............................................................................................................8 System commands from inside Open GENIE.........................................................9 GETTING HELP........................................................................................................... 11 THE THREE WISHES .............................................................................................12 A SIMPLE EXAMPLE.................................................................................................. 12 THE FIRST WISH - ACCESS TO DATA......................................................................... 16 Accessing raw data spectra .................................................................................16 Accessing ASCII files...........................................................................................18 THE SECOND WISH - TO DISPLAY DATA................................................................... 20

Opening a graphics device. ...................................................................................................... 20 Displaying a graphical plot of spectra from a workspace......................................................... 20 Performing a multiplot of 2-D spectra on the same x-axis....................................................... 22 Overplotting an existing graph................................................................................................. 23 Altering the graphics parameters in the Display(), Plot() and Multiplot() commands ............. 23 Magnify a portion of the plot chosen interactively................................................................... 25 Plotting data from an ASCII file .............................................................................................. 25

Making alterations.................................................................................................................... 27

Display a cursor on the graphics screen to allow annotation.................................................... 28

To save a hardcopy of the graphics into a file.......................................................................... 29

Procedures................................................................................................................................ 29

THE FINAL WISH - TO MANIPULATE DATA............................................................... 30

Mathematical functions .......................................................................................30

Workspace operations..........................................................................................32

Data Analysis Functions......................................................................................35

The Open GENIE Module Interface....................................................................39

What is a module?.................................................................................................................... 39

When would I want to use modules?........................................................................................ 39

How do I write a module.......................................................................................................... 39

1. Write FORTRAN Subroutines to do your tasks................................................................... 40

2. Write a FORTRAN �wrapper� subroutine to interface betweenOpen GENIE and your calculation subroutine.............................................................................................................. 40

3. Make the Module Library .................................................................................................... 42

4. Load the module into Open GENIE..................................................................................... 42

5. Package function arguments into a workspace..................................................................... 42

6. Execute the module and get the result.................................................................................. 43

A Real-Life Sample Module.................................................................................................... 43

The C Module Interface........................................................................................................... 46

Example Open GENIE programs ........................................................................50

FURTHER DEVELOPMENTS AND ADVANCED PROGRAMMING..................................... 54

THE END OF PART I................................................................................................... 55

PART B - INSTALLATIO N GUIDE.......................................................................56

INSTALLINGOPEN GENIE........................................................................................56

BINARY INSTALLATION............................................................................................. 57

SOURCE CODE INSTALLATION................................................................................... 60

Operating system specific notes...........................................................................62

Linux........................................................................................................................................ 62

IRIX......................................................................................................................................... 63

VMS......................................................................................................................................... 63

APPENDICES ............................................................................................................64

APPENDIX A ............................................................................................................. 64

Features of the command line..............................................................................64

Additional features................................................................................................................... 64

APPENDIX B.............................................................................................................. 65 Supported Data File Formats ..............................................................................65 APPENDIX C.............................................................................................................. 66 Supported Graphics Devices ...............................................................................66 APPENDIX D ............................................................................................................. 67 Supported Graphics Attributes ............................................................................67

Fonts ........................................................................................................................................ 67 Markers .................................................................................................................................... 67 Linestyles................................................................................................................................. 67 Colours..................................................................................................................................... 68

APPENDIX E.............................................................................................................. 69 Commands required for installing Open GENIE from a CD ROM.....................69

Installing on UNIX with Digital UNIX.................................................................................... 69 Installing on VMS.................................................................................................................... 69

PartA - User Manual

What is Open GENIE ?

GENIE is the name of a programs used for the display and analysis of data from the neutron scattering instruments at the ISIS facility. For several years now, a stable VAX/VMS version of the software (GENIE-V2) has been in use atISIS

(Rutherford Appleton Laboratory, Oxfordshire, UK), and at several scientific and commercial establishments world-wide. Constant improvements in the capabilities of the neutron scattering instruments at ISIS, and in the hardware and software available for data analysis, has necessitated a re-write of GENIE. The new GENIE is known as

Open GENIE to reflect the intention that the software be used on a wide variety of different computers and operating systems. It is aimed at supplying scientists with an inexpensive computer package which provides them with access to their experimental data, so that they may analyse the data as required and display the results in a useful format, usually in a graphical form.

Getting Started

If you are new toOpen GENIE, we recommend that you work through �The Three

Wishes� section of theUser manual. This should give you a clear idea of what facilities Open GENIE provides and how to use them. After this working through one or two of the examples programs should provide sufficient knowledge to enable you to work with Open Genie. For the more experienced GENIE user, a brief read of the

User manual is recommended to determine the differences between older versions of

GENIE, and the new revised Open GENIE.

2

Starting up Open Genie

Remote operation of Open GENIE at ISIS

a) Via Telnet Firstly telnet into one of the main VMS server machines ptath, horus, or thoth using >telnet ptath.nd.rl.ac.uk If you want to use the graphics you will need to set the X display back to your local machine $set display/create/tran=tcpip/node=your.own.machines.ip.address and start Open GENIE by typing $opengenie

b) Via a terminal emulator If you start remote sessions on a UNIX workstation via a terminal emulator such as eXceed or eXcursion, you can start Open GENIE directly by telling �rexec� to run the �rgenie� command. Note the full pathname may be required, for example >/usr/local/bin/rgenie

 The �rgenie� command can take several parameters, for further details type

       >man rgenie

 A typical use may be to startOpen GENIE with your own �genieinit.gcl� file, for

example

 >rgenie �myinit.gcl�

An alternative is to use the terminal emulator to set up an xterm or a decterm on one of the UNIX or VMS workstations from which Open GENIE can then be run.

A few useful facts about Open GENIE

Commands

Commands in GENIE are entered via the command line. The command line is based on the GNU readline library and you will find that you can recall and edit previous commands by using the arrow/cursor keys. Commands are saved between sessions in a �.genie_history� file in your home directory, and this can be searched for previous commands. For features of the command line see the appendix A.

Commands in Open GENIE consist of either assignments or keyword commands.

Assignments are made using the �=� sign, for example

<destination-location>=<expression>

The destination-location is a variable or an element of a compound variable such as an array or workspace, and the expression can be:

• a literal value e.g. 5.6 or �hello�

• a variable or part of a variable e.g.Two_theta, or w1.npts

• function expression e.g. Sin($Pi)

• unary or binary expression e.g.-1, or 1+2

Any Open GENIE procedure can be implemented by akeyword command, and if the procedure returns a value it can also be invoked in an expression, where the value is assigned to a variable. A keyword command starts with a keyword followed by a list of qualifiers and parameters. The keyword specifies the basic command, while the qualifiers modify the action of the command and theparameters supply the values which the command operates on. For example, a keyword command is

>>display/Line w1

This command plots the workspace w1 as a line. By itself the display command plots a histogram, the /line qualifier modifies the command to perform the plot as a line

Data types may be eitherconstants or variables. Constants are prefixed by a �$�, and can only have a value assigned to them once, usually when they are first created. All available constants can be viewed by typing:

>>Show/Const

System constants are prefixed by $_ and can be viewed with

>>show/const/sys

Variables are created by assigning a value to an unused variable name. A variable name may consist of alphanumeric characters, the �_� character, or numbers, but must start with a letter. Examples are

>>A=2.0 ; B=6

To see all the defined variables type:

>>Show/Var

All variables are preceded by an underscore �_� are reserved for internal use byOpen

GENIE and these may change or be removed at any time, and therefore you should avoid using any variable starting with �_�. The command

>>Show/Var/Sys

will show all system variables.

Arrays are structures that contain more than one variable. There are three array types one for each of the basic variable types. An array is created by first generating an empty array of the appropriate size and dimensionality using theDimensions() function and then by assigning values to its elements. For example

# Create a RealArray

>>two_d_data = Dimensions(100,200) # created in 2-dimensions

>>two_d_data[1,1] = 5.0            # type is set here to real

>>Printn two_d_data

[5.0 _ _ _ _ ...] Array(100 200 )

Arrays may be manipulated as a whole or, alternatively, individual elements may be accessed and modified separately. Note: all elements which have not had a value

assigned to them are marked as _. You can specify a value for undefined elements using the FIX() command.

Workspaces are compound variables, where individual elements of the variable maybe of different types (contrast with arrays, which are all of one type). Examples of similar structures in other languages are arecord in Pascal or a struct in C. The following example shows the construction of a simple workspace interactively.

#  create a brand new workspace
>> mywork = fields()    # creates an empty workspace
>> Printn mywork        # look at it now
Workspace []
(
)
>>
# Now put some fields in it
>> mywork.description = "My test workspace"
>> mywork.some_value = 3.14159
>> mywork.anarray = dimensions(2,3)
>> mywork.anarray[1,1] = 25
>> Printn mywork         # now look again
Workspace []
(
some_value = 3.14159
anarray = [25 _ _ _ ...] Array(2 3 )
description = "My test workspace"
)
>>

Note: structure() may be used instead of fields().

Operations

The normal operations on integers and real numbers are

• x^y. If x is an integer then the result will be an integer no matter whether y is fractional or not.

• +, -, *, /, and the remainder or modulo function |. For the quotient and remainder operations on integers the convention is to truncate towards zero.

• <, >, =, <=, >=, !=. The comparisons of: less than and greater than, equal to, less than or equal to, greater than or equal to and, not equal to respectively.

• Sin(x), Cos(x), Tan(x), Arcsin(x), Arccos(x), Arctan(x). The trigonometric functions, where x is quoted in radians. The constant $PI is available for conversion to degrees.

• Log(x), Ln(x), Exp(x) the Transcendental functions.

Note: the results of the trig. and transcendental operations on integers are given as real numbers, and when an expression contains integers and real numbers the result is given as real after implicitly converting any integer values to corresponding real values.

The normal operations on strings are:

• + or & concatenates two strings. For example,

>>A= �Hello� + � there� & �!�

• <, >, =, <=, >=, !=. For strings of the same length, the comparisons act as a test based on the collating order of the text in the strings. For strings of different lengths, comparisons are between the string lengths.

• Substring(), Locate(), Length() for more information see String

Handling Functions in the Reference Manual.

The basic operations on arrays are those of the corresponding data type plus:

• Array[i,j,k,...]. This indexing allows individual array elements to be accessed using integer indices. Note: all indices start at one. For example

>>printn my_array[12,34,5,3,2]

32

• Array[l1:l2,l3:l4,...]. This slicing of an array produces a smaller array with limits of l1 to l2, l3 to l4. If variables are used as limits extra brackets must be included. For example

>>a=my_array[2:4,4:100]
>>b=another_array[(i):(k)]

• & Appends the RHS array to the end of the LHS array, for this operation both arrays must be of the same variable type.

Note: the unary, trig. and transcendental functions are applied individually to each element of the array. The binary operations are applied to the elements of the two arrays, if the arrays differ in dimensionality, the corresponding elements are selected using storage order. The result of the operation is to create a new array of identical structure to the array on the left hand side of the operator. If the LHS array is longer, the extra elements are set to the undefined value nil in the result array, while if the LHS array is shorter the result array is truncated to the length of the LHS array. The comparisons test whether the elements and/or length differ.

The basic operations on workspaces are those of the corresponding data type plus:

• <workspace>.<field-name>. This field accessing allows its value to be read or set. A field is automatically created in a workspace when a value is assigned to it.

The comparisons when operated on workspaces assume that the workspace is anOpen GENIE spectrum, but these operations can be modified by the user, see theOpen GENIE reference manual.

File names

Open GENIE takes file names in either the VMS style or UNIX style depending on the system being used. For VMS

USER$DISK:[FAA.GENIE]TEST.DAT

or on UNIX

/usr/users/cmm/genie/test.dat

System commands from inside Open GENIE

The cd command changes the default working directory while inOpen GENIE. For example:

# Change to the examples directory on UNIX

>>cd �/usr/local/genie/examples�

>>dir

Note: the directory path is as specified on the native operating system, e.g. VMS or

UNIX.

The dir command lists the files in the current directory or the directory specified on the host operating system. For example:

# List the examples directory on VMS

>>dir �[.examples]�

The pwd prints the current working directory. For example

# Change to the examples directory

>>cd "/usr/local/genie/examples"

>>pwd

/usr/local/genie/examples

The Os command prints the operating system Open GENIE is currently running. For example:

# Print the current operating system

>>printn Os()

OSF

The system command allows you to execute a single command or a command session of the native operating system from withinOpen GENIE. For example:

# find some user details on VMS

>>system �SEARCH journal.txt \�flux\� �

IRS14142ZAB/NJR Flux tests  18-FEB-1997 12:00:01 163.2

IRS14143ZAB/NJR Flux tests  18-FEB-1997 13:43:40   6.1

>>

If no command is given as a parameter, the System() command starts a sub-shell process which is terminated by an exit on UNIX, or a LOGOUT on VMS systems. Note

that on VMS some normal logical name definitions may be missing in the sub process.

Getting help

Online Help in Open GENIE is available in a number of ways:

• to see a list of all Open GENIE commands , press <Ctrl>H on a blank command line; if it pressed after a letter a list of all commands that start with that letter will be printed

• pressing <tab> twice will list all commands that match with what has already been typed so far. Therefore pressing <tab> twice on an empty command line lists all the commands.

• if the command name is not known use <Ctrl>K to perform a keyword search of the command descriptions

• if the command name is known, run it with the /HELP qualifier to get a description and list of parameters. For example

>> display/help

The Three Wishes

Most people using Open GENIE will wish to do one of three things

Wish 1 - Access their data, either from a file or directly from the data acquisition electronics.

Wish 2 - Display their data on the screen and make a hardcopy on a printer.

Wish 3 - Manipulate their data, for example, to focus or normalise it.

These are described separately in the following sections, but first this�.

A Simple Example

Below is a description of a simple Open GENIE session to access time of flight data taken on the High Resolution Powder Diffraction (HRPD) instrument which gives you some idea of the usage of Open GENIE commands.

$opengenie
Open GENIE V1.0 BUILD-23 [Linked] Thu Jan 2 15:26:39 GMT 1997
[library version] 1.0(Running on alpha:VMS:6.2 (built with DEC
C++ V5.3))
>>

for UNIX systems use

>genie

Now that Open GENIE is running, most people will wish to set up some defaults to allow easy access to files in the data area of the instrument they are using. If you always use one instrument, these defaults can be set up in a command file to be run automatically when Open GENIE starts. Normally Open GENIE looks for the file �genieinit.gcl� in your home directory, so the defaults can be placed in that file

>>set/disk �axplib$disk:�
Default disk: axplib$disk:
>>set/instrument �hrp�
Default instrument: hrp

>>set/directory �[OPENGENIE.GENIE.EXAMPLES.DATA]�

Default directory: [OPENGENIE.GENIE.EXAMPLES.DATA]

>>set/extension �raw�

Default filename extension: .raw

On UNIX, the commands for setting defaults are similar and use the appropriate syntax for UNIX file names, except no Set/Disk command is needed. However, on all operating systems it is essential to put string arguments in double quotes.

>>set/instrument �hrp�

Default instrument: hrp

>>set/directory �/usr/local/genie/examples/data/�

Default directory: /usr/local/genie/examples/data/

>>set/extension �raw�

Default filename extension: .raw

Any raw set of data can then be collected using the Assign command followed by the run number

>>assign 8639

Default input: /usr/local/genie/examples/data/hrp08639.raw

An alternative is to use the Set/File/Input command which explicitly sets the file to be used. For example,

>>Set/File/Input �/usr/local/genie/examples/data/hrp08639.raw�

Default input: /usr/local/genie/examples/data/hrp08639.raw

Now that the source for the data has been selected individual spectra can be extracted from the data set using the spectrum function, which can be normally abbreviated to

�s�.

>>w = s(7)

Reading spectrum 7 /usr/local/genie/examples/data/hrp08639.raw

>>noise = s(1)

Reading spectrum 1 /usr/local/genie/examples/data/hrp08639.raw

>>corrected = w - noise

Here the seventh spectrum is read into the workspace w. The first spectrum in the file is subtracted from the spectrum in w and the result is put into the workspace

corrected. The corrected spectrum can now be displayed on a graph using the
display command, and the binning number altered to 10

      >>alter/binning 10

from within Open GENIE you will be told where Open GENIEis installed, and from that you can deduce the position of the examples directory.

The First Wish - Access to Data

At ISIS and all other neutron scattering centres data is collected in �runs�. These are typically periods of time in which the sample is kept in constant conditions. The data for a run is stored in a raw data file, and at ISIS the naming convention is <instrumentxxxx.raw>, where the run number is xxxx. The raw file itself contains one or more time-of-flight spectra and other associated parameters needed for the analysis of the data. This section describes the commands necessary to access data fromOpen GENIE. The description that follows is based on the data formats found at ISIS. However Open GENIE can be modified to read other formats used at other facilities. This section details all the commands used to access data from Open GENIE.

Accessing raw data spectra

One of the major strengths of Open GENIE is the flexibility available in accessing data. The first way of accessing data is based on the old GENIE-V2, where several internal variables control the

a) current input file,

b) current output file,

c) current disk,

d) current directory,

e) current instrument,

f) current file extension

The status of these variables is changed by using the set() command (detailed on page 12). The show/defaults command gives the input/output defaults, for example

>>show/defaults
Current default disk = AXPLIB$DISK:
Current default directory = [OPENGENIE.GENIE.EXAMPLES.DATA]
Current default instrument = HRP

Current default extension = .RAW

Current default input =

AXPLIB$DISK:[OPENGENIE.GENIE.EXAMPLES.DATA]HRP08639.RAW

Current default output =

>>

To read a spectrum or multiple spectra from a raw data file the assign and

spectrum () commands can be used. An alternative to this is to use the Get()

command. The Get () command is able to read data from either a raw data file, or another of the supported data formats, see Appendix B. However, this assumes that the data items in a file are either named explicitly, or numbered. For example, the data read from a raw data file could be a spectrum or a user name. The most useful parameters, which can be taken from a raw data file are TITL, the run title; USER, the user information; NAME, the instrument name; NDET, the number of detectors; TTHE, the two theta table; NSP1, the total number of spectra; NTC1, the number of time channels;

LEN2, L2 for each detector, and each individual spectra file are specified by an

associated integer, i.e. specifying 5 would get the fifth spectra from within a file. For example:

# print the user name

# then read in all the spectra in the file,

# finally read every third spectrum from a file

>>printn get(�USER�,

�/usr/local/genie/examples/data/hrp08639.raw�)

WIFD/RMI

>>d2 = get(1 : get(�NSP1�))

>>spin_up =get(1:50@3)

Note: if a file has been set using the Set/File/Input command then if no file is stipulated it defaults to this file.

To save Open GENIE variables to an intermediate binary file the Put() command is used. These variables may optionally be tagged with a label, which can be used for later reading, or comments may also be added. For example,

# Copy a whole multidimensional spectrum from a raw file into a
single item in an intermediate file

>> Set/File/Input �/usr/local/genie/examples/data/irs12839.raw�

>> Set/File/Output �example.in3�

>> Put get(1:20) label = �bigspec� comment = �demo�

which can then be read with

>> get (�bigspec�)

Accessing ASCII files

To read in data from an ASCII file, for example from the file �prs_001.obs�, which can be found in the PRISMA directory of the Open GENIE example area

# Read in three data arrays of 30 points (in columns separated
by a whitespace)
# and assign to arrays in fields X, Y, and E in the new
workspace.
>>handle=Asciifile:Open(�/usr/local/genie/examples/prisma/prs_0
01.obs�)
>>wk1=Asciifile:Readfree(Handle, �X,Y,E�,$whitespace, 30)
>>printn wk1
  Workspace []
  (
    x = [0.925 0.975 1.02499999999999 1.07499999999999
1.125...] Array(30 )
    y = [0.22526098 0.11728537 0.126243569999999
0.144312439999999 0.15559034 ...] Array(30 )
    e = [0.009967181499999 0.0043424088 0.004095190999999
0.003976735 0.0038093579 ...] Array(30 )
  )
>>

or alternatively

>>Asciifile/Readfree Handle �X,Y,E� $whitespace 30
>>wk1=Asciifile:data(handle)
>>

The second method enables several different items of data to be accumulated into a workspace before it is returned. For example:

>>Asciifile/Readfree Handle "X1,Y1,E1" $WHITESPACE 4
>>Asciifile/Readfree Handle "X2,Y2,E2" $WHITESPACE 4
>>wk1 = Asciifile:data(Handle)
>>printn wk1
  Workspace []
  (
    x1 = [1.0 1.1 1.2 1.3 ] Array(4 )
    y1 = [2.1 2.1 2.2 2.0 ] Array(4 )

    e1 = [0.0 0.1 0.2 0.0 ] Array(4 )

    x2 = [1.4 1.5 1.6 1.7 ] Array(4 )

    y2 = [2.0 2.0 2.0 2.0 ] Array(4 )

    e2 = [0.1 0.1 0.2 0.0 ] Array(4 )

  )

Note: you can also use the Put/Ascii command to output data to an Asciifile.

Other commands concerned with the input and output of data can be found in the

Open GENIE reference manual.

The Second Wish - To Display Data

Opening a graphics device.

Examples of the use of many of these commands may be found in thegcl procedures in the /usr/local/genie/examples directory on ISIS UNIX systems or

AXPLIB$DISK[OPENGENIE.GENIE.EXAMPLES] on ISIS VMS.

Before you can plot any data, you need to select a device on which to display the data.

>>Device/open �device-type� width height

The default device is an X-window �XW�. Other supported devices include �TEK4010� Tek 4010 compatible, �PS� postscript, �CPS� colour postscript, and �HPGL� HPGL driver for 7475A. For full details of the supported devices on each machine see the supported graphics devices in appendix B. The size of the page (in inches) is defined by the width and height parameters the default value is taken to be 8 inches. Alternatively you can open a device with a name:

>>device1=Device:Open (type, width, height)

This is useful as Open GENIEsupports multiple open devices, a given window can then be selected using the Select command. For example

>>Select Device1

Displaying a graphical plot of spectra from a workspace.

After the data has been read into a workspace from aRAW file or intermediate GENIE file, the data can then be plotted using the display command. The plot will be automatically scaled and titled with other relevant information from the workspace. For example:

# Display a spectrum but change the title first
>>wm = s(10)
>>wm.title = �This is my Nobel plot!�
>>display wm 0 100 -35 70

Alternatively you can plot it directly using

>>display s(10)

which displays the 10_{th} spectra of the default input file, or alternatively use the Get () command

>>Display get(10,�hrp00273.raw�)

The parameters after the workspace wm are respectivelyxmin, xmax, ymin, ymax. All the parameters, except for the workspace, are optional and where omitted a default value will apply. Specifying a keyword for each parameter allows you to define each individual limit. For example, if the X limits should be defaulted, but the Y limits defined, then you could use:

>>Display wm ymin=-35 ymax=70

The parameters may also be expressions using functions of variables, for example

>>Display w1-noise 0 xmax/100.0 ymin=Min(w1.y) ymax=Max(w1.y)

Anonymous placeholders may also be used to indicate a default value - inOpen

GENIE the character �_� is used. The above example could then be written as

>>Display w1 _ _ -35 70

>>

Other optional parameters that may be specified are:

Linecolour - the colour for drawing the axes and surrounding boxes,

Linewidth - the line width used for drawing line plots,

Textcolour - the colour used for drawing text.

Other qualifiers:

/HISTOGRAM - displays as a histogram assuming that the binned data has one

more X value than Y value.

/LINE - displays a spectrum as if it is a numerically calculated function (i.e.

with the same number of X-values as Y-values) and join the points with straight lines. Note: if histogram data is displayed with the /Line qualifier, the data will be transformed to take the bin centre positions as the X-values for the data points, this is done with the Centre_bins() function.

/MARKERS - displays a plot with markers symbols. For a list ofmarker types

see appendix D.

/ERRORS - display as error bars taken from the workspace error array.

In order to clear the display surface on the currently open device:

>>Device/Clear

While

>>Device/Close

deactivates the currently open graphics device.

Performing a multiplot of 2-D spectra on the same x-axis

This is done using the Multiplot command, and it is useful for comparing groups of spectra from different detectors. A pseudo Y-axis is produced where successive plots are placed with an artificial Y offset value (ygap). Currently, multiplot only plots as a histogram. If used to plot a spectra from a raw file then the data source for the multiplot can be specified using the Set/File command. For example:

# Do multiplots from a file
>>multiplot 1:20 file = �mydata.raw" ygap=10.0
>>multiplot 1:300@3    # plot every third spectrum

Optional parameters (note the types) are: Linecolour (Colour), Linetype (LineStyle), Linewidth (Real), Textcolour (Colour1), Textheight (Real).

Overplotting an existing graph

This is done using the Plot command, which does not have the ability to create axes or scale the data.. For example:

#Plot a vanadium spectrum on top of

#the data as a comparison

>>Display s(5) xmin=20000.0

>>Plot/Line get("vanadium1","normal.in3")

Qualifiers: /Histogram, /Line, /Markers, /Errors

Altering the graphics parameters in the Display(), Plot() and Multiplot() commands

Modifying characteristics of the plot is achieved using the commands Alter(),

Toggle(), or Limits().

Alter/Status Reports the values of all settings.

Alter/Binning Sets bin grouping for plotting. If the bin grouping value is

set to a value greater than one, the display command groups the data by averaging the values ofn-bin groups. It is possible to apply the same operation to a standard workspace permanently using the Groupbins() command.

Alter/Device Changes the interactive device.

Alter/Font Sets the text font for all the text used in the display.

Alter/Hardcopy Changes the default hardcopy device, when a Hardcopy()

command is issued.

Alter/Linecolour Changes the axes and box colour

Alter/Linetype Changes the line style for line plots

Alter/Linewidth Changes the overall line thickness

Toggle/RY Y axis rounding off/on

Toggle/Info Informational message printing on/off

[/On] Toggles item on

[/Off] Toggles item off

For example:

# Switch off informational messages and display

# a data plot with no banner heading.

>> Toggle/info

>> Toggle/header

>> Display s(22)

The limits of the graph can be changed using the Limits() command. For example:

# Set the limits before doing a display

>> Limits/X xmin=10.0E4 xmax=50.0E4

>> Display # Redisplays previous plot with new limits

The command Limits/Default clears this. Note the actual setting of the limits will still be dependent on whether rounding is switched on for the X-axis.

Magnify a portion of the plot chosen interactively

This is done using the Zoom command, which redraws a plot scaling to a box which is selected by the cursor (the lower left-hand corner and the upper r.h corner of the box).

The qualifiers /Errors, /Histogram, /Line, /Markers, will redraw the plot using error bars, histograms, lines, or markers respectively. While the /Multiplot qualifier expands a region of a multiplot. For example:

# Zoom in on the current plot

# and re-display with error bars

>> zoom/errors

Plotting data from an ASCII file

In this example the data used is prs_001.obs, which can be found in the directory of

�../genie/examples/prisma�. To construct a plot if you have read in a nonOpen

GENIE type file, e.g. an ASCII "X,Y,E" file intow.x, w.y, w.e, then after opening a new graphics device using

>>Device/Open

a window must be created with the Win_ commands. In this case a Scaled or AutoScaled window is created by

>>Win_Scaled 0.1 0.9 0.1 0.9 0.975 7.475 0.02 0.17

The first four numbers define the device co-ordinates - the position of the plotting box on the page, and the last four numbers are the global co-ordinates - the X and Y range of the plot. The points of the graphical device range from 0.0 and 1.0. By using the

Win_Autoscale command, and quoting the x and y arrays in the parameter list the

range of the plot are chosen automatically; for example:

>>Win_Autoscaled 0.1 0.9 0.1 0.9 w.x w.y w.e $Red

where w is the workspace containing the data, and the $red parameter will paint the chosen window red instead of the default black.

Now we can create the graph

>>Graph/Draw w.x w.y

green axes can be drawn by

>>axes/draw colour=$green

By default the axes are linear, and the x and y axes are labelled horizontally and vertically respectively. To display x/y labels on the graphics device

>>labels/draw �X Axis� �Y Axis�

To draw text on the graphics device

>>text/draw 0.0 1.0 �some text� colour=$yellow size=3.0
angle=45.0 font=$script

the position is specified in world co-ordinates.

To display a title on the graphics device

>>title/draw �A Title�

Comparing this data with the data from the file prs_001_lmf.cor (after loading the

ASCII data file into the w1.x, w1.y and w1.e) plot the data with markers as blue crosses

>>markers/draw w1.x w1.y $Blue $Cross 2

To include Y error-bars

>>errors/draw/Vertical w.x w.y w.e $Blue 2

and to draw a green graticule on the window

>>graticule/draw colour=$green

Note: for a complete list of qualifiers associated with these commands see the Open

GENIE reference manual.

To ensure the above picture and its associated objects can be referred to later, after a new picture has been created then initially a picture should be created,

>>picture1=Picture()

and then the following commands used

>>scaled1=Win_Scaled(0.1,0.9,0.1,0.9,0.975,7.475,0.02,0.17)

>>graph1=GRAPH:DRAW(w.x, w.y)

>>axes1=axes:draw(colour=$green)

>>labels1=labels:draw(�X Axis�, �Y Axis�)

>>text1=text:draw(0.0, 1.0, �some text�, colour = $yellow
size=3.0, angle=45, font = $script)

>>title1=title:draw(�A Title�)

>>markers1=markers:draw(w1.x,w1.y,$Blue,$Cross,2)

>>errors1=errors:draw:Vertical(w.x, w.y, w.e $Blue 2)

>>graticule1=graticule:draw(colour=$green)

Now to view this plot open a new device

>>device1=device:open()

>>Redraw picture1

Making alterations

If you wish now to change part of the graphs for example the text in picture1

# Want the font to be italic
>>title/alter font=$italic object=title1

or you want to change the graticule

>>graticule/alter colour=$red object=graticule1

In order to remove the changes caused by the/draw qualifier the Undraw command can be used. For example, if you wanted toundraw markers1 then type

>>Undraw markers1

Note: if the Undraw command is followed by a negative integer,N then it is the previous N^{th} Draw that is undone. In other words, Undraw -1, undoes the previous

Draw command (the default); whereas Undraw -3 undoes the command two before

the last one.

For a whole set of pictures and opened devices made for examplepicture1, picture2 picture3 picture4 etc. and device1, device2, device3, device4, etc., then to redraw picture4 on device5, and picture 6 on device2 then type

>>Redraw picture4 device5
>>Redraw picture6 device2

In order to redraw a previous plot then type

>>Redraw -1

After a number of device:open() commands have been executed then to redraw the current picture on the current device type

>>Redraw 0.

Display a cursor on the graphics screen to allow annotation

This is done using the Cursor command. An obvious use is for tagging peaks with the data value in the X or Y direction at the point selected by the cursor. For example

# Display a cursor near the expected position
# of a peak in world co-ordinates.
>>Cursor/Horizontal 10000.0 50.0

# If /vertical is used instead then the text is drawn
vertically

a cursor is displayed and waits for a pressed key, if X - displays �X co-ordinate�; Y - displays �Y co-ordinate�; P - displays both co-ordinates; T- to add text; and E-exit.

See also the GetCursor command in the Open GENIE reference manual.

To save a hardcopy of the graphics into a file

The Hardcopy command allows a copy to be made of either the currently displayed window, or an earlier picture to a postscript file. For example:

# Save a copy of the last but one picture as

# colour postscript (found with Redraw/Info)

>>Hardcopy filename = �test.cps� picture = my_pict

The default name of the file into which the hardcopy is placed is �GENIE.PS�. The filename extension is one of the supported hardcopy graphics devices. For full details of supported devices on each machine type see the appendix. The default picture selected is 0 - the last picture created. Normally just typingHardcopy is sufficient to make a hardcopy of the current screen.

Procedures

A whole series of graphics commands can be strung together and stored as a procedure. See for example the various directories of /usr/local/genie/examples.

The procedures are then loaded using the command

>>Load �File.gcl�

and executed using the command

>>File

The Final Wish - To Manipulate Data

This section can be separated into three distinct areas

• mathematical functions

• workspace operations

• data analysis functions

Mathematical functions

As well as providing intrinsic arithmetic operations for different data typesOpen

GENIE provides several basic functions for performing mathematical operations.

These are coded generically so that the same function can be applied to any data type which is capable of undergoing the operation. For example, the Sin() function may be used on a single number, an array or a workspace. Normally, the result of the operation is of the same data type as the value operated upon. Where the operand contains several values (e.g. an array), each value is operated on individually. For example we can create an array of real numbers, and square root them

>>my_numbers = Dimensions(10,20) # First create a 10 x 20 array

>>fill my_numbers 1.0 1.0       # Fill the array with some data

>> printn my_numbers

[1.0 2.0 3.0 4.0 5.0 ...] Array(10 20 )

>> printn sqrt(my_numbers)       # print the square roots.

[1.0 1.414213 1.732050 2.0 2.236067 ...] Array(10 20 )

The basic mathematical functions are

• trigonometric functions - with the angle in radians

Arccos(), Arcsin(), Arctan(),Cos(), Sin(), Tan(). For example,

# print result in degrees

>>y = Arccos(0.5) * 180 / $pi

# take the arccos of all elements in an array

>>a = Dimensions(10)      # create a 10 element array

>>fill a 0.5              # Set all elements to 0.5
>>y = Arccos(a)

• transcendental functions

Exp(), Ln(), Log(). For example,

# antilog a data array
# which is in logs to base 10
>>data = Exp(w.y*ln(10.0))

• other functions

Abs()^1, Sqrt(). For example:

# Calculate the square root of Pi
>>printn Sqrt($PI)
1.77245310234149

1 Abs() calculates the absolute value of a number or of the numbers in an array. All negative numbers will be returned as positive numbers of the same magnitude.

Workspace operations

Workspace operations and transformations form the heart of Open GENIE. These allow analysis of the data taking into account its underlying form. For example, the

Units() command can be used to convert the units of a time-of-flight (TOF)

spectrum. This is only possible if some assumptions are made about the fields which are present in the workspaces containing the experimental data. For the Units() command to work, a workspace also requires fields giving parameters such as the primary flight path and incident angle (a TOF spectrum).

For example for a 2-D TOF Spectrum needs

Workspace Field Description Variable type

X(1-D) array of X values RealArray

Y(2-D) 2-D array of Y values RealArray

E(2-D) 2-D array of errors for Y field RealArray

L1 primary flight path (m) Real

L2(1-D) secondary flight path (m) Real array

Twotheta(1-D) scattering angle (degrees) Real array

Delta hold off in microseconds Real

Emode energy mode Integer 0=inelastic, 1=incident,

2=transmitted

Efixed fixed energy (if applicable) Real

Xlabel Units for X values String

Ylabel Units for Y values String

Ut(1-D) User parameters (this array may be of any length and caters for information not already named in a field)

RealArray

For more on the necessary fields required for operations then see theOpen GENIE reference manual.

Template routines are called whenever an intrinsic operation involving workspaces is specified. In most cases the errors are propagated through the calculation. The template routines on workspaces are:

• Unary operations

Trigonometric and transcendental functions. For example

w2=ln(w1) is equivalent to w2=workspace_ln(w1)

and

Workspace_arccos(w) is equivalent to acos(w),

Other unary functions

Workspace_sqrt, sqrt(w); Workspace_abs, |w|; and,
Workspace_negated, -w.

• Binary Operations

Workspace_add(), w1+w2; Workspace_append (joins one end of one

histogram to another), w1&w2, Workspace_divide, w1/w2;

Workspace_raised_to, w1^w2; Workspace_subtract, w1-w2;
Workspace_modulo, w1|w2; Workspace_multiply, w1*w2.

The characteristics (i.e. final length, dimensionality of arrays) of the left hand workspace define those of the resultant workspace.

• Comparison Operations

Workspace_equal, w1=w2;

Workspace_not_equal, w1!=w2.

The definition of the default routines are stored in the file �workspace_user.gcl�, which is included in the library directory of theOpen GENIE distribution.

Data Analysis Functions

Arguably the most important purpose ofOpen GENIE is as a tool for scientific data analysis. Not just for preliminary data analysis, but as a framework which provides, or from which can be called, all the tools necessary to perform a complete analysis of the data.

Currently, a large amount of data analysis is performed with a set of disparate FORTRAN programs which have to support their own routines to access data, to drive a user interface and to work with a variety of different graphics packages. What is critical and is very much at the heart of the philosophy ofOpen GENIE is that the scientist must have control over is how the data is processed.

A scientist may trust the Open GENIE peak fitting routines, alternatively and probably more the case at the moment, the scientists will want to continue to use their own analysis code in a C or FORTRAN subroutine for most things.Open GENIE can be used to provide the user interface, graphics and file access. This mechanism is described fully in the next section of this manual on modules, and these allow the code to be run as if it was a compiled part of Open GENIE. Routines which have been found to be useful in several different areas of analysis are hard coded in C/C++ or FORTRAN for efficiency.

The current routines available are:

• Focus()

Focus a range of time of flight spectra from detectors at different scattering angles with given parameters. This command, although written specifically for focusing multiple banks of detectors consecutively can be used for single scanning detectors data. To focus the spectra in d-spacing (with the :D switch), or in momentum transfer (with the :Q switch) the time of flight parameters are required, which can be specified from a file (the default are the values from the raw file). Note: the default is the :D switch where spectra are summed in d-space. For example:

# Focus a time of flight spectrum in D-spacing
# get the TOF parameters from the raw data file

>>w = focus( 1:17, �irs12838.raw� )

# Focus default file, every third period

>>assign 3045

>>refl = focus(3:90@3, _, mydet)

• Integrate()

Integrate a 1-D or 2-D spectra. For example:

# print the integrals of two spectra

>> printn integrate(1:2, 38000, 78000, "tfx00345.raw")

INTEGRATE: Integrating between 38000 and 7800

  Workspace []

  (

    error = [2341.4700 1027.1312 ] Array(2 )

    sum = [5482585.0 1054968.0 ] Array(2 )

  )

The result of the integrate command is returned as a workspace with two fields: the

�SUM� field contains either a single value or an array of integrals, and the �ERROR� field contains the propagated error of the result.

• Peak()

Provides interactive peak fitting of a workspace allowing selection of the bounds of the peak and the form of fit to use. The available fits for use are:

1.Gaussian - a Gaussian-peak sitting with a straight-line background,

2.Gaussian convoluted with an exponential - a Gaussian convoluted with a sharp-edged exponential, sitting on a straight-line background,

3.Lorentzian - a Lorentzian-peak, sitting on a straight-line background,

4.Lorentzian convoluted with exponential - a Lorentzian convoluted with a sharp-edged exponential, sitting on a straight-line background,

5.Voigt - a Voigt convoluted with a sharp-edged exponential, sitting on a straight-line background,

6.Polynomial - fits an n_{th} degree polynomial,

7. Voigt convoluted with an exponential - a Voigt convoluted with an exponential.

Once fitted the peak parameters of the fit are displayed and made available as a result, so that they can be used later. For example:

# Fit peaks from a genie intermediate file
>>fit = peak( get(3, �mydata.in3�))
>>printn fit

Note: See the Peakfit() and Peakgen() in the Open GENIE reference manual for more control and detail.

• Rebin()

The rebin command performs an interpolation from one histogram into another histogram with the same integrated count, but with modified X-boundaries. Some numerical precision is lost during a re-binning operation and there is usually a degree of peak broadening, so multiple re-binning is to be avoided. The /Lin and /Log qualifiers allow a Linear or Logarithmic rebinning between the specified boundaries to be performed. For linear rebinning the boundaries are specified in steps, for logarithmic bin widths these are calculated such that for any given binning range

X_{n+1} - X_n = Step * X_n

For example, given the command

>>w = rebin:log(w, 10.0, 0.1, 15.0)

Here the step is 0.1, and the range of the rebinning is between 10 and 15. The bin boundaries generated will be [10, 11, 12.1, 13.31, 14.641, 15].

A workspace can also be rebinned according to another workspace. For example:

# Read a spectrum and re-bin the same as an
# already loaded vanadium workspace
>>w=s(1)
>>w=rebin(w, vanadium.x)

• Units()

This command converts the units of time-of-flight spectra. Using the switches they can be converted respectively to:

/C or /Channel to Channel numbers (one way)

/D To D-Spacing (A)

/E To Energy (meV)

/LAM To Wavelength (¯)

/Q To Momentum Transfer (¯_{-1})

/SQ To (Momentum Transfer)_2(A_{-2})

/T To Time of Flight (μs)

/LA1 To primary flight path wavelength

/W To energy transfer E1-E2 (meV)

/WN To energy transfer E1-E2 (cm_{-1})

/TAU To reciprocal time-of-flight (μs/m)

For example:

# Read in a spectrum whilst converting to Wavelength

>>w = units:Lam(s(1))

The t.o.f parameters must be set correctly in the input workspace (or set using the

Set/Par command) in order to perform the conversion, and if the keyword syntax is

used, i.e. Units/C w the workspace will be converted destructively.

1. Write FORTRAN Subroutines to do your tasks

The subroutines can take any parameters you desire. Our example will be based on the subroutine �myfunc.for� in the examples directory:

2. Write a FORTRAN � wrapper� subroutine to interface between Open GENIE and your calculation subroutine

Open GENIE variables are passed to and from the module using a temporary workspace. Data is placed into the input workspace with chosen field names, and then accessed in FORTRAN by using this field name and an access routine appropriate for the data type being sent. For example, theframe count could be stored in the variable

�NRAW� and accessed using themodule_get_int() function in FORTRAN.

Returning data is similar - the various module_put() FORTRAN subroutines allow the construction of a returned workspace containing various data types with named variables. The wrapper subroutine must obey the following rules:

• It must be a SUBROUTINE taking just two parameters, calledPARS_GET and

PARS_PUT. These parameters should be declared EXTERNAL and not be accessed in

anyway, except via �module_...� commands.

• It must allocate the variables needed by the user�s SUBROUTINE and transfer data to/from them using �module_get_...� and �module_put_..� calls.

• As input/output devices are re-assigned byOpen Genie, READ(5,*) commands should be avoided and screen output should be handled via the �module_print�

C

C *** The function - just square the X array

C

      SUBROUTINE MYFUNC(X, Y, NPT)

      IMPLICIT NONE

      INTEGER NPT, I

      REAL X(NPT), Y(NPT)

      DO I=1,NPT

      Y(I) = X(I) * X(I)

      ENDDO

      RETURN

      END

and �module_information� commands. Inside the moduleOpen GENIE variables are accessed by workspace field names. For example, in the program below the array X is loaded from the field labelled �XVALS�, where it has been placed by a GCL procedure. There is no restriction on how you label a variable, but often you will use the variable name itself. All �module_get_..� routines must specify

Pars_Get as the first parameter, and similarly all �module_put...� routines

specify Pars_Put (these variables are, in fact, just references to the input/output parameter workspaces of the Module/Execute command.

For a full list of module_.() functions see the FORTRAN module interface in the Open GENIE reference manual.

For our example �myfunc� the wrapper would be:

C *** the wrapper subroutine for MYFUNC
C *** input into array X, output into array Y
C
      SUBROUTINE DO_MYFUNC(PARS_GET, PARS_PUT)
      IMPLICIT NONE
      INTEGER NPT_MAX, NPT
C *** We can handle NPT_MAX data points
      PARAMETER(NPT_MAX=1000)
      REAL X(NPT_MAX), Y(NPT_MAX)
      EXTERNAL PARS_GET, PARS_PUT
C *** print a "blue" message to the user
      CALL MODULE_INFORMATION(�Inside module --- MYFUNC called!!!�)
C *** Set NPT to the max. size of the array
C *** On return, NPT will be the number of data points passed
      NPT = NPT_MAX
C *** The input was placed in a workspace field called ’XVALS’ in GCL
      CALL MODULE_GET_REAL_ARRAY(PARS_GET, ’XVALS’, X, NPT)
      IF (NPT .GT. NPT_MAX) THEN
      CALL MODULE_ERROR(�myfunc module�, ’Too many points�, � �)
      RETURN
      ENDIF
      CALL MYFUNC(X, Y, NPT)
C *** now return the result (Y) in a workspace field called ’YVALS’
      CALL MODULE_PUT_REAL_ARRAY(PARS_PUT, ’YVALS’, Y, NPT)
      RETURN
      END

3. Make the Module Library

You need to compile the file containing the function and its associated wrapper using the Module/Compile command - this will produce a �.so� file to load intoOpen

GENIE.

>>Module/Compile �myfunc.for� Symbols = �do_myfunc�

This command first runs a FORTRAN compiler on the code, then it produces a shared library from the object code. If the compilation fails for any reason you will see various error messages on the screen and the creation of the shared library will be aborted. On a successful run, you will see a message similar to the following:

** Module now compiled - load with: Module/Load �myfunc.so�

The Symbols parameter must be set to a comma separated list of wrapper subroutines that you wish to call from Open GENIE (via Module/Execute).

4. Load the module into Open GENIE

To load the module, use Module/Load command with the name of the �.so� file created by the Module/Compile. You can also supply a comment that will be displayed when you later typeModule/List.

>>Module/List �myfunc.so� �My function module!�

You only need to reload a module if you change the source code and have executed another Module/Compile command.

5. Package function arguments into a workspace

You now need to create a workspace to hold the parameters for the Subroutine you wish to call in the module. The fields in the workspace must have the same names as those you specified in the second argument of your �module_get...� calls above. In our case, we only have one variable and we called it �XVALS�, so assuming X is the array we wish to send:

>>X=Dimensions(10) # create a new array

>>Fill X 1.0 1.0 # Fill array with numbers 1.0 to 10.0

>>Pars=Fields() #create an empty workspace for module arguments
>>Pars.Xvals = X # add X to workspace as field �Xvals�

6. Execute the module and get the result

This is achieved by:

>>MY_RESULT = Module:Execute(�my_func�, Pars)

where �my_func� is the name of the FORTRAN wrapper routine you wrote, andPars is the packaged arguments workspace created above. The values specified in �module_put..� calls will appear in the returned workspaceMY_RESULT; in the above case MY_RESULT will contain one entry called YVALS, so we can type:

>>Printn MY_RESULT.YVALS

and see squared X values!

A Real-Life Sample Module

The following module was created by Spencer Howells at ISIS - the code is available in the �ex2� subdirectory of the examples area asg2s.gcl and g2s.for.

First the GCL procedure that calls the module:

# Procedures for G2S
#
PROCEDURE g2s
PARAMETERS
wg = workspace
RESULT ws
LOCAL g2s res
ws = wg
g2s=fields() ; g2s.lptin=wg.ntc
g2s.Xin=wg.x ; g2s.Yin=wg.y ; g2s.Ein=wg.e
g2s.qmax=inquire("g2s> qmax ")
g2s.npt =inquire("g2s> number of points ")
g2s.ic =inquire("g2s> window function code ")
g2s.rho =inquire("g2s> number density ")
module/load "g2s.so" ;
res=module:execute("g2s", g2s)
ws.ntc=res.lptout
ws.x=res.Xout ; ws.y=res.Yout ; ws.e=res.Eout

ws.xlabel=res.xcaptout ; ws.ylabel=res.ycaptout

ENDPROCEDURE

Now the FORTRAN program that performs the actual calculation:

      SUBROUTINE G2S(g2s_get, g2s_put)

      EXTERNAL g2s_get, g2s_put

      INTEGER mn, lptin, lptout

      PARAMETER (mn=33000)

      REAL*4 Xin(mn),Yin(mn),Ein(mn),Xout(mn),Yout(mn),Eout(mn)

      REAL*4 xnew(mn),yw(mn)

      CHARACTER*40 xcaptout, ycaptout

      CHARACTER*10 char

      LOGICAL LMOD

      DANGLE=38.1*1.112/150.0/150.0

      PI=4.0*ATAN(1.0D0)

      call module_get_int(g2s_get, ’lptin’, lptin)

      call module_get_real_array(g2s_get, ’Xin’, Xin, lptin)

      call module_get_real_array(g2s_get, ’Yin’, Yin, lptin)

      call module_get_real_array(g2s_get, ’Ein’, Ein, lptin)

      call module_get_real(g2s_get, ’qmax’, QMAX)

      call module_get_int(g2s_get, ’npt’, npt)

      call module_get_int(g2s_get, ’ic’, ichar)

      call module_get_real(g2s_get, ’rho’, RHO)

      if(lptin.eq.0)then

        call module_error(� G2S�, 1 �ERROR ** No input data�, � �)

      endif

      if(npt.eq.0)then

      call module_error(�G2S>�,1�ERROR No of output points zero�,� �)

      RETURN

      endif

      lptout=npt

      if(lptout.GT.mn)then

      call module_error(� G2S>�, 1 �#points reduced from 33000�, � �)

      lptout=mn

      endif

      delq=QMAX/lptout

      if(rho.lt.1e-10)then

      call module_error(� G2S>�, 1 �ERROR ** rho is zero�, � �)

      RETURN

      endif

      if(ichar.eq.0)then
      LMOD=.false.
      else
      if(ichar.eq.1)then
      LMOD=.true.
      else
      LMOD=.false.
      endif
      endif
      if(LMOD)then
      A=PI/xin(lptin)
      do nn=1,lptin
      yw(nn)=SIN(xin(nn)*A)/xin(nn)/A
      end do
      else
      do nn=1,lptin
      yw(nn)=1.0
      end do
      endif
C
C FORM VECTOR OF EQUALLY-SPACED R’S AT WHICH THE FOURIER TRANSFORM C
IS TO BE COMPUTED (RMAX IN ANGSTROMS), AND THE NUMBER OF R-POINTS.
C
      DO NR=1,lptout
      xout(NR)=delq*NR
      end do
C
C THE NUMBER OF POINTS IN THE RANGE OF DATA TO BE TRANSFORMED.
C
      xd=(xin(2)-xin(1))/2. !half x-channel
      do n=1,lptin
C xnew(n)=xin(n) +xd !offset - mid channel
      xnew(n)=xin(n)
      yw(n)=yw(n)*(yin(n)-1.)*xnew(n)
      end do
C
C COMPUTE FOURIER TRANSFORM OF THE DATA
C
      delr=(xin(lptin)-xin(1))/(lptin-1)
      AFACT=delr*2.0/PI
      DO 35 NR=1,lptout
      FS=0.0
      RP=xout(NR)
      DO N=2,lptin
      SINUS1=SIN(xnew(N-1)*RP)
      SINUS=SIN(xnew(N)*RP)

      FS=FS+ (SINUS*yw(N)+ 1 SINUS1*yw(N-1))/2.0

      end do

      yout(NR)=FS*AFACT

35    CONTINUE

C

      pir=PI*PI*2.*RHO

      do n=1,lptout

      yout(n)=yout(n)*pir/xout(n) +1.

      end do

      xcaptout=� Q (Angstrom-1)� ycaptout= � Structure Factor S of Q�

      call module_put_int(g2s_put, �lptout�, LPTOUT)

      call module_put_real_array(g2s_put, �Xout�, Xout, lptout)

      call module_put_real_array(g2s_put, �Yout�, Yout, npt)

      call module_put_real_array(g2s_put, �Eout�, Eout, npt)

      call module_put_string(g2s_put, �ycaptout�, ycaptout)

      call module_put_string(g2s_put, �xcaptout�, xcaptout)

      call module_information(� G2S> output is in point mode�)

      RETURN

      END

The C Module Interface

The C module interface is used in almost exactly the same way as the FORTRAN interface, and provides similar routines - in fact most have the same name but with a prefix of cmodule_ rather than module_. Invoking from the GCL command line is similar, except that an extra qualifier of /C must be specified for COMPILE and

EXECUTE operations (it could also be specified on a load for consistency, but is not strictly necessary). For example,

>>MODULE/COMPILE/C �myprog.c�

>>MODULE/LOAD �myprog.so�

>>VALS=MODULE:EXECUTE:C(�myfunc�, PARS)

The major difference between the two is in the arguments - the C module routines can allocate memory for returned array structures usingmalloc(), unlike in FORTRAN77 where a pre-allocated array must always be passed. To indicate that you wish a routine to allocate the memory for you, set the array pointer to NULL before passing the address of it to the routine. For example:

GenieWorkspace *pars_get, *pars_put; /* passed from GENIE */
const char* name = �twotheta�; /* parameter to get */
fort_real* val_array =NULL; /*tell routine to malloc() memory*/
fort_int len;
/* then get array the array*/
cmodule_get_real_array(pars_get, name, &val_array, &len);

/* do some manipulations and return new values */
cmodule_put_real_array(pars_put, name, val_array, len);
free(val_array); /* release storage */

If a pointer is not NULL, the routine will assume it points to valid storage of size �len� - on return, �len� will be set to the number of elements of the array actually set, or 0 on an error. A C module must contain the following header files

#include <genie_cmodule.h>
#include <genie_cmodule_ver.h>

to set up the correct definitions and typedefs.

The MODULE/COMPILE/C Open GENIE command will insert the correct path for picking up these header files, but they are contained in the $GENIE_DIR/library directory if you wish to peruse them

The C module function must be declared like:

void my_cmodule(GenieWorkspace* pars_get, GenieWorkspace*
pars_put);
{
if (!cmodule_version_ok(CMODULE_MAJOR_VERSION,
CMODULE_MINOR_VERSION))
{
cmodule_print(�Library version mismatch in MY_C_MODULE�,
CMODULE_PRINT_ERROR);
return;
}
/* all OK, proceed */
}

Variables are obtained and set by calling the following functions, with eitherpars_get or pars_put and the variable name: (taken from

Genie_Dir/library/genie_cmodule.h)

/* Get REAL parameter NAME from GENIE as VAL */
void cmodule_get_real(GenieWorkspace* pars_get, const char*
name, fort_real* val);

/* Return REAL variable VAL to GENIE as NAME */
void cmodule_put_real(GenieWorkspace* pars_put, const char*
name, fort_real val);

/* Return DOUBLE variable VAL to GENIE as NAME */
void cmodule_put_double(GenieWorkspace* pars_put, const char*
name, fort_double val);

/* Get STRING parameter NAME from GENIE as VAL

This routine ALWAYS allocates space for val with malloc(),
and you will need to free() at a later stage*/
void cmodule_get_string(GenieWorkspace* pars_get, const char*
name, char** val);

/* Return STRING variable VAL to GENIE as NAME */
void cmodule_put_string(GenieWorkspace* pars_put, const char*
name, const char* val);

/* Return STRING array VAL of LEN elements to GENIE as NAME */
void cmodule_put_string_array(GenieWorkspace* pars_put, const
char* name,const char* val[], fort_int len);

/* Get INTEGER parameter NAME from GENIE as VAL */
void cmodule_get_int(GenieWorkspace* pars_get, const char*
name, fort_int* val);

/* Return INTEGER variable VAL to GENIE as NAME */
void cmodule_put_int(GenieWorkspace* pars_put, const char*
name, fort_int val);

/* Get REAL array parameter NAME from GENIE as VAL

On Input:

The routine will malloc() space for the array if (*val ==

NULL),otherwise it will assume *val points to an array of size
len

On Output:

On error, *len will be set to 0

Otherwise, *len will be set to the number of elements read into

*val

*/
void cmodule_get_real_array(GenieWorkspace* pars_get, const
char* name, fort_real** val, fort_int* len);

Example Open GENIE programs

The basic commands of Open GENIE plus multiline commands, for example IF -

ELSE - ENDIF statements can be combined into gcl procedures. Below is a list of

examples, these are arranged, so that the programs can be easily run byOpen GENIE test routines, or by someone trying to get an idea of whatOpen GENIE can do. Most programs have their own directory, with the data required taken from files stored in this area_1.

If program fails to link, change into the example directory and type

>make links

this will usually find the appropriate data files and set up the appropriate �data� directory link.

It is best that these programs are load and run from the appropriate directory. For example, using the the file dopamine.gcl in the directory

/usr/local/genie/examples/simple_graphics. Firstly change to this directory,

and then load the program using

>>Load �dopamine.gcl�

and run these programs using the name of the file, in this case

>>dopamine

Before running most of the programs you will have to execute adevice/open command.

• Analysis focus_example.gcl - this example puts the necessary defaults into a workspace, that is required for focusing data from an IRIS raw data file.

1 For large data files a link is made in the program directory to an external data area to avoid keeping large files in the source tree, however the access remains the same.

integrate_example.gcl - integrates a single spectra and a set of single spectra rebin_example.gcl - rebins the data to the same range, but different number of time channels, then integrates the spectra. The procedure then rebins to a given X range, to a set of given X values, and to linear steps in a given range and then integrated. The data is then rebinned using logarithmic steps and integrated.

• Contour contour_test.gcl - draws a filled colour contour plot, and then overplots two sets of contour lines, • IRIS add.gcl - procedure to analyse IRIS diffraction data. Developed by P. Marshall • Data This directory holds the data used for some of the procedures in the examples section. • ex1 dssdemo.gcl - this demonstrates the use of different plot styles, with error bars and line plots of linear and logarithmic scales. • io contains various examples of programs concerned with the input and output of data from genie. ascii_file.gcl - demonstrates the use of Open GENIE routines to read/write ASCII data using the ASCIIFILE command. ascii_io.gcl - demonstrates the use of Open GENIE routines to output and input data in a fixed easy reading ASCII file format using theGet and Put command intermediate_file.gcl - gives an example of the use of the Open GENIE routines to manipulate intermediate files.

raw_file.gcl - example of the use of Open GENIE routines to read and manipulate spectra from ISIS raw files

• modules

This directory gives examples of wrapping routines -c_example.gcl and fortran_example.gcl - for the calling of a module from within Open GENIE written in gcl, and examples of a such modules for C and FORTRAN- c_example.c and fortran_example.f

• newget

In this section examples are given of C, C++, and FORTRAN files, which can be used like the get() function of Open GENIE. • peak pktest.gcl - a procedure which generates data from a quadratic equation and then fits a cubic equation to the data, with the linear part of the function inputted by the user and then held constant. The data, the fit and the residuals are then plotted.

• prisma diffuse.gcl, phon.gcl - examples of publication graphics by Mark Harris. Loads ASCII data from a file creating a graph and plotting observed and theoretical data as markers and lines respectively.

• report report.gcl - this procedure demonstrates the ability to read data using an external

FORTRAN program, and the use of CONTOUR and CELL_ARRAY commands in making a colour contour plot on data taken on MARI.

• simple_graphics boxes.gcl - this procedure draws boxes on the plot window with corners chosen by the operator.

dopamine.gcl - this procedure reads in a .PRO file. It then plots two ranges of observed data as points with the calculated data plotted as a line. The difference between the calculated and data plot below. The data file OPT17.PRO was obtained from a Rietveld fit of a structural model of deuterated dopamine hydrobromide to HRPD data.

funcplot.gcl - this plots a function of your own specification by writing a module �on the fly� and then using this module to generate the data points

test_mutitplot.gcl - a procedure which produces a multi-plot from a spectra, and then Examples of multiplots constructs a multiplot from a 2-D array

textcirc.gcl - draws the string �A simple text string� in a circle.

• slides

slides.gcl - this procedure is a slide demonstration of Open GENIE�s main features.

• two_d_graphics

contour_test.gcl - displays a contour plot of a set of neutron inelastic spectra taken on IRIS.

glad.gcl - draws a colour intensity map of S(Q, ω) data taken on MARI, which also allows you to see slices of the intensity variation with constant energy, and momentum.

Further Developments and Advanced programming

A Tk Tcl Interface is currently under development at ISIS, and the idea is to provide a rudimentary interface and also a set of useful utilities e.g. a tcl �display� command that will, as well as drawing a plot, allow you to interactively change e.g. line colour by clicking on a line. However, the above should allow anybody who wishes the ability to knock up a GUI for a GCL command procedure they write.

Open GENIE is a much more detailed and powerful system than is obvious from the rest of this manual. There are many things which can be done usingOpen GENIE, for example write procedures in an object oriented command syntax extend the data class system to advanced data types code procedures directly insmalltalk or extend Open GENIE by writing in C++

The End of Part I

At the end of a session all variables created during it are lost when

>>Exit
GENIE exiting
$

is typed.

However, all the variables from one Open GENIE session can be saved into a binary image file. This is useful when a number of gcl procedures have been loaded, and will mean you don�t have to typeLoad �procedure.gcl� next time. This is achieved using the save()

>>Save �my_saved_session�

The session can be re-started by the command

genie � �my_saved_session�

The � are needed because the first argument can be used to load up agcl file on startup, instead of $HOME/genieinit.gcl. Thus you are able to define commands for different start-ups, for example

VMS: marigenie :== opengenie sys$login:mariinit.gcl

UNIX C shell: alias marigenie �genie $HOME/mariinit.gcl�

Part B - Installation Guide

Installing Open GENIE

Open GENIE is available as a binary distribution for the common machine types and in a source code distribution for anything else. If the binary distribution is available for your machine and operating system, this is the easiest way to installOpen GENIE.

The binary distribution kits are marked with the name of the machine, the operating system and the manufacturer of the machine range if known. For example

alpha-dec-osf3.2

means that the version of Open GENIE in the binary distribution was made for a machine with an alpha/AXP processor, in a machine manufactured by Digital

Equipment Corporation and running Version 3.2 of the OSF/1 operating system, which is now called Digital UNIX. In general all these should match with your system for a binary kit to work. If you are running a version of UNIX, but are unsure of these details you can download the file �config.guess� directly from the ISIS website at http://www.isis.rl.ac.uk/GenieUsermanual/config.guess website, and run it on your system with the command

>sh config.guess

This script will attempt to guess which version of UNIX you are running and return a string similar to the one above. If it matches one of the GENIE binary distributions this will be the appropriate version to use for your machine.

Installation instructions for VMS and UNIX machines are different so there are different sections describing how to install each one. If your machine does not have a binary version of the kit available, you may be able to build one from the source code, to do this you will need to read the section on Source code installation. Note for example instructions to mount the CD-ROM see appendix E.

Binary Installation

Choose the binary installation instructions below which match the type of hardware on which you are installing Open GENIE.

a) UNIX Installation All UNIX kits are supplied as compressed tar files - made by the tar program on the appropriate machine. To decompress these files you will need to havegunzip installed. NB gunzip is available from the web site as a tar file if you do not have this, for building on your system.

To install Open GENIE follow the instructions given here for a Digital Alpha machine, but substituting the appropriate names and version numbers for your distribution kit of Open GENIE gunzip genie-1.1-alpha-dec-osf3.2.tar.gz tar xvf genie-1.1-alpha-dec-osf3.2.tar cd genie-1.1-alpha-dec-osf3.2 To install GENIE in the default system location with data files in

/usr/local/genie, executable files in /usr/local/bin, and library links in
/usr/local/lib type:
 ./configure
 make install

You will need to do the make install from the superuser or root account. If you wish to see what make install will do without actually performing the install, type make -n install Note: the above install can only be executed by the superuser and does a system wide installation. If you do not have access to the superuser account, you may

change the ./configure command to give different default installation directories for yourself, for example

./configure --prefix=$HOME will change the default installation directories, putting any binary files into your personal account�s$HOME/bin directory, the rest of genie into a$HOME/genie directory, and library symbolic links in$HOME/lib. Note: to run Open GENIE automatically yourbin directory will need to be in yourPATH.

Once Open GENIE is installed it can be invoked by running the genie script in the bin directory. If thebin directory is specified in your shellPATH environment variable, you should be able to just type:

 genie

If you are using a C shell then before the command will work properly you need to type:

 rehash

b) VMS Installation

Below are the steps needed to get Open GENIE running on a Dec alpha/AXP machine running VMS6.2 or later.

All VMS/alpha kits are supplied as compressed zip files, made by the public domain zip program. To decompress you will need to haveunzip installed. If unzip is not installed by default on your system then to set up the command type the following line:

$unzip :== $ disk:[directory]unzip_axp.exe where disk:[directory] is the location of the unzip_axp.exe file (this is available from the Open GENIE web pages).

Uncompress the Open GENIE kit using the command below (you will need approximately 40000 blocks of disk space to successfully uncompress and install

Open GENIE):

 $unzip genie-1_0-alpha-dec-vms6_2.zip

This creates a directory called disk:[directory.OPENGENIE_1_1]. To run Open GENIE you will need to set up the definition

$opengenie :== @disk:[directory.opengenie_1_1]genie_setup

either your own �LOGIN.COM� or the system wide �SYLOGIN.COM�. This enables Open GENIE to be run using the command opengenie. For installing Open GENIE on a system which is shared between several users you may want to install the shared library and executable files as known shareable images. This is done by adding the lines

 $INSTALL ADD disk:[directory:OPENGENIE_1_1.GENIE]genie.so
/OPEN/HEADER/SHARED/RESIDENT

$INSTALL ADD disk:[directory:OPENGENIE_1_1.GENIE]GMAIN

/OPEN/HEADER/SHARED/RESIDENT

to the SYSTARTUP_VMS.COM file in SYS$STARTUP.

c) WindowsNT & WINDOWS 95 installation

Windows/NT and Windows-95 are currently not supported, but will be made available in subsequent releases.

Source Code Installation

Unless you are fully prepared to compile a fairly complex software system written in

C/C++ we recommend that you check for a binary installation ofOpen GENIE and install that instead.

Source code installation is normally more complicated than the Binary installation, but it is useful if:

a) you need to install Open GENIE on a machine/operating system combination for which we have not yet provided a binary installation.

b) you wish to develop or modify theOpen GENIE code in some way.

It is also very likely that you will need to have some familiarity with the C, C++ and

FORTRAN compilers on your system. Generally we would recommend that you install GNU g++ and use either g77 or the native FORTRAN compiler for building

Open GENIE.

Before embarking on a source code build, it may well be worth mailing us at genie@isise.rl.ac.uk to check that we are not planning to do a similar build or that someone else has not already done one.

The source code is distributed in a compressed tar file which you will need to unwind in a suitable development area. The PGPLOT and Splash libraries are distributed as separate distributions which will need to be unpacked in PGLOT and Splash subdirectories respectively. We have to do this becauseOpen GENIE is being distributed under the GNU licence, and the other packages though freely available are not. Following this the trees must be patched to update them with modifications and files added for Open GENIE. The commands needed will be similar to the ones shown below.

cat genie-1.1.tar.gz | gunzip | tar xf -
cd genie-1.1
cat ../pgplot5.1.1.tar.gz | gunzip | tar xf -
cd splash
cat ../../splash1.7.tar.Z | gunzip | tar xf -

The pgplot tree should now be in the �pgplot� subdirectory andsplash in the �splash� subdirectory. The patches can be applied with the commands

cd genie-1.1/pgplot
patch -p2 -s < pgplot-5.1.1.patch
cd ../splash
patch -p2 -s < splash-1.7.patch

These patches should apply fully without asking questions, if you get a question such as �File to patch:�, check thatpgplot and splash were extracted correctly, so that the paths genie-1.1/pgplot/makemake and genie-1.1/splash/Makefile.in both point to valid files.

Ideally, the code will now build automatically if you type.

cd genie-1.1
./configure
make all

this builds the development version of Open GENIE which can be run by typing

./parser from within the src directory. To go the whole way and build an install kit

for your system you will need to do a

make kit

to build a compressed tar file for a binary installation. This can then be installed to a users directory or system wide as described in the section onBinary Installation. Note that to build a kit you will also need a copy of GNU autoconf installed (see

ftp://ftp.nd.rl.ac.uk/pub/packages/gnu).

If you are struggling emailgenie@isise.rl.ac.uk and we will endeavour to help. When you do contact us for advice, please provide us with examples of the errors that occur in the mail message. Remember that we probably can only guess at what might be wrong as we are unlikely to have the same system that you have to test things on.

Please check out the operating system specific notes below, they could save you a lot of time!

Operating system specific notes

At the moment our primary development platform is Digital UNIX (OSF/1) on alpha AXP and this is generally the one which works best for building without a hitch.

Linux works fine, but may need a bit of fiddling if you run a different distribution to us. IRIX (for version 5.3) works, but is likely not to work immediately for later versions. For VMS, only attempt this if you are strong willed and familiar with

VMS/POSIX and have it installed on VMS 6.2 or later. VMS building on VAX is not recommended although we have done it!

We provide notes to help you with building on specific operating systems, these notes can also be found in the README.<os> files of the source code distribution.

Linux

This is not an exhaustive list but should help:

1. One version of g++ on the Linux we build on (1.2.13) does not find its own include files by default. Before building define the include path with export CPLUS_INCLUDE_PATH=/usr/include/g++-include

2. It may also be necessary to editsrc/Makefile and remove the flag - extend_source from the $(F77) rule

3. After the first build attempt,

 $cd library

 $make -i

Note g77 return status of 4 stops a correct build

4. cd src and touch lexcommands.c. To ensure that flex doesn’t overwrite this with unworking code.

5. go into pgplot and edit the makefile to remove -f2c from the begining of the

"LIBS=" line. Re-make to build the pgxwin_server properly

6. Now try �make all� again, it should run through this time. IRIX First run ./configure, currently this picks up f2c if it is installed which is probably not what is wanted. Now edit �./config.cache� and change the line

f2c_c_cos=${ac_cv_lib_f2c_c_cos= �yes�}

to read

f2c_c_cos=${ac_cv_lib_f2c_c_cos= �no�}

and re-run configure. VMS These are the instructions for compiling under VMS POSIX, tested on Open VMS (AXP) 6.2 with POSIX 2.0. Before entering VMS POSIX:

DEFINE/JOB POSIX$INCLUDE SYS$SCRATCH

After entering POSIX:

sh vms_posix.setup

will building the kit using a fairly large number of rather VMS/POSIX specific routines and produce a similar file to the UNIX versions. In general it is possible that if the configure doesn�t work then it may be the result of picking the wrong FORTRAN compiler. To change this you can edit the file �config.cache� and then re-run the configure command.

Appendices

Appendix A

Features of the command line

• Pressing <TAB> on a partially completed command will complete the command if it is unambiguous, otherwise pressing <TAB> a second time will list possible options.

• Pressing <TAB> also works for partially completed file/directory paths

• Pressing <Ctrl>H on a partially complete command will give a one line summary of all commands matching that pattern

• Pressing <Ctrl>K will start a �command keyword� help search - type in a one word query, and all commands whose description matches this will be printed

• Pressing <Ctrl>R will start an incremental reverse search of previously typed commands

• Pressing <Ctrl>L will clear the screen and redraw the current line at the top

Additional features

• Pressing <Ctrl>_ will undo a last edit/change you made to the command line

• Pressing <Ctrl>X<Ctrl>U will also undo the last edit/change

• Pressing <Ctrl>U will discard the rest of the line starting from the current cursor position

• Pressing <Ctrl>A will move the cursor to the beginning of line

• Pressing <Ctrl>E will move to end of the current line

Appendix C

Supported Graphics Devices

Below is a list of graphics devices currently supported byOpen GENIE, these rely upon the PGPLOT package and it may well be possible to use other pgplot drivers with Open GENIE. In the distributed version of Open GENIE we have only checked out the functioning of the devices below on all platforms. To see other devices which may be available on a particular version ofOpen GENIE type

>> Device/Open �Help�

Device Name Description String

Tcl/Tk driver �TK� or �tk�

X-Windows devices �XWINDOW� or �xw�

Postscript (portrait) �PS� or �ps�

Colour Postscript (portrait) �CPS� or �cps�

Postscript (landscape) �PS� or �ps�

Colour Postscript

(landscape) �VCPS� or �vcps�

Appendix D

Supported Graphics Attributes

Fonts

Open GENIE uses the PGPLOT fonts when drawing fonts onto the open graphics device, currently, the supported fonts available are:

$NORMAL
$ROMAN
$ITALIC
$SCRIPT

Note: For accessing special scientific/Greek characters within these fonts, the documented PGPLOT escape sequences may be used in theOpen GENIE text string being plotted. For example �Time-of-Flight (\gms)� where �\gm� produces a Greekμ character. For further details see the PGPLOT documentation, available at

ftp://astro.caltech.edu/pub/pgplot.

Markers

Markers types available for plotting.

$POINT
$PLUS
$STAR
$CIRCLE
$CROSS
$BOX

Linestyles

Linestyles available for plotting.

$FULL
$DASH
$DOT_DASH
$DOT

Colours

Pre-defined colours available for the graphics by default. For using further colours in the graphics, see the Open Genie reference manual.

$BLACK

$WHITE

$RED

$GREEN

$BLUE

$CYAN

$MAGENTA

$YELLOW

$ORANGE

$LIGHT_GREEN

$SEA_GREEN

$LIGHT_BLUE

$PURPLE

$CRIMSON

$DARK_GRAY

$LIGHT_GRAY

Appendix E

Commands required for installing Open GENIE from a CD ROM

Please note that these commands vary depending on the version of the operating system you are using. Installing on UNIX with Digital UNIX Initially find the CD

>file /dev/rrz*c

and look for an RRD device e.g. RRD42 on /dev/rrz4c then mount the CD

>mount -t cdfs -o ro,rrip /dev/rz4c /mnt

then get the kit

>cp /mnt/osf/genie-1.1.31F

Note: you will need to have the CDFS kernel option enabled. Installing on VMS Type in, for example

$mount DKA400:GENIE11
$copy sys$scratch: /log